# HackTV Info

#### TECHNICAL DATA

&CODE: | ACTIVATED | DESCRIPTION
&vers | &vers; | Client Version
&wtv-bootvers | &wtv-bootvers; | Boot Version
&wtv-syscfg | &wtv-syscfg; | System Configuration
&wtv-chipvers | &wtv-chipvers; | Chip Version
&wtv-ssn | &wtv-ssn; | Silicon Serial ID #
&rate | &rate; | Modem Speed
&wtv-appvers | &wtv-appvers; | Client Build
&cpu | &cpu; | CPU Speed
&wtv-vidinfo | &wtv-vidinfo; | Video Decoder
&wtv-scrres | &wtv-scrres; | Screen Resolution
&wtv-1800addr | &wtv-1800addr; | WNI Server IP

#### BROWSER SETTINGS

&CODE: | ACTIVATED | DESCRIPTION
&thumb | &thumb; | Thumbnail URL
&find | &find; | Contents of your "FIND" box
&wtv-adv-opt | &wtv-adv-opt; | Advanced Options
&url | &url; | URL of current page
&exurl | &exurl; | Last URL visited
&title | &title; | Title of current page
&date | &date; | Current Date - use set clock.
&fsize | &fsize; | font size: small, medium or large
&kbd | &kbd; | On-screen keyboard config: alphabetical or standard
&brdrs | &brdrs; | Shade of screen border
&wtv-muzac-on | &wtv-music-on; | ?
&tempo | &tempo; | Music Tempo
&connpw | &connpw; | Connect to web when powering on
&vol | &vol; | background music volume: setup-bgm-volume

#### PHONE SETUP

&CODE: | ACTIVATED | DESCRIPTION
&audio | &audio; | Audible dialing
&pulse | &pulse; | Pulse dialing on/off
&tone | &tone; | Tone dialing on/off
&dtone | &dtone; | Wait for dial tone
&hack | &hack; | Call waiting on/off
&nowait | &nowait; | No callwaiting
&wtv-sens1 | &sens1; | call waiting sensitivity
&wtv-sens2 | &sens2; | call waiting sensitivity
&wtv-sens3 | &sens3; | call waiting sensitivity
&wtv-sens4 | &sens4; | call waiting sensitivity
&slow | &slow; | Dialing Speed
&med | &med; | Dialing Speed
&fast | &fast; | Dialing Speed
&outstr | &outstr; | Dialing prefix from wtv-setup:/phone-basic
&wstr | &wstr; | Call waiting block prefix from wtv-setup:/phone-call-waiting
&phone | ☎ | Your phone #. This has worked periodically
&ldp | &ldp; | Long distance dialing prefix
&free | &free; | 1-800 number override
&anum | &anum; | Special Dialup # from file://rom/htmls/AccessNumber.html
&hasit | &hasit; | ?
&dout | &dout; | ?
&broke | &broke; | ?

#### BYOISP SETUP

&CODE: | ACTIVATED | DESCRIPTION
pname | &pname; | BYOISP provider name
&lname | &lname; | ISP user login name
&banum | &banum; | BYOISP Dialup 1
&banum2 | &banum2; | BYOISP Backup Dialup. May be blocked.
&bpass | &bpass; | BYOISP password. May be blocked.
&byoisp | &byoisp; | BYOISP

#### PLUS TV SETUP:

&CODE: | ACTIVATED | DESCRIPTION
&tv-zip | &tv-zipcode; | ZIP for TV listings. Set at TV Home
&tv-download | &tv-download; | AutoRetrieve of TV listings. Set at TV Home
&tv-dl-time | &tv-dl-time; | AutoRetrieve time of TV listings. Set at TV Home
&tv-cable | &tv-cable; | Using cable TV? Set at TV Home
&tv-antenna | &tv-antenna; | Using TV antenna? Set at TV Home
&tv-satellite | &tv-satellite; | Using satellite system? Set at TV Home

#### DISHPLAYER ONLY

&CODE: | ACTIVATED | DESCRIPTION
&sat-nfo-rid | &sat-nfo-rid; | reveiver ID
&sat-nfo-cid | &sat-nfo-cid; | smartcard ID

#### MISC.

&CODE: | ACTIVATED | DESCRIPTION
&brdre | &brdre; | ?
&mod | &mod; | Last Modified Date? but always says 1969 or 1970 if clock isn't set.
&legalese | &legalese; | Either "invisible" or left blank. Have no idea what this does.
&ext-videoin | &ext-videoin; | Extension video inputs?
&size | &size; | ?